Home · Quickstart · Documentation · Citation · NiPy

# interfaces.mrtrix.preprocess

## DWI2Tensor

Link to code

Wraps command dwi2tensor

Converts diffusion-weighted images to tensor images.

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> dwi2tensor = mrt.DWI2Tensor()
    >>> dwi2tensor.inputs.in_file = 'dwi.mif'
    >>> dwi2tensor.inputs.encoding_file = 'encoding.txt'
    >>> dwi2tensor.cmdline
    'dwi2tensor -grad encoding.txt dwi.mif dwi_tensor.mif'
    >>> dwi2tensor.run()

Inputs:

    [Mandatory]
    in_file: (an existing file name)
            Diffusion-weighted images
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    encoding_file: (a file name)
            Encoding file supplied as a 4xN text file with each line is in the
            format [ X Y Z b ], where [ X Y Z ] describe the direction of the
            applied gradient, and b gives the b-value in units (1000 s/mm^2).
            See FSL2MRTrix()
            flag: -grad %s, position: 2
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    ignore_slice_by_volume: (a list of from 2 to 2 items which are an
             integer)
            Requires two values (i.e. [34 1] for [Slice Volume] Ignores the
            image slices specified when computing the tensor. Slice here means
            the z coordinate of the slice to be ignored.
            flag: -ignoreslices %s, position: 2
    ignore_volumes: (a list of at least 1 items which are an integer)
            Requires two values (i.e. [2 5 6] for [Volumes] Ignores the image
            volumes specified when computing the tensor.
            flag: -ignorevolumes %s, position: 2
    out_filename: (a file name)
            Output tensor filename
            flag: %s, position: -1
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1

Outputs:

    tensor: (an existing file name)
            path/name of output diffusion tensor image

## Erode

Link to code

Wraps command erode

Erode (or dilates) a mask (i.e. binary) image

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> erode = mrt.Erode()
    >>> erode.inputs.in_file = 'mask.mif'
    >>> erode.run()

Inputs:

    [Mandatory]
    in_file: (an existing file name)
            Input mask image to be eroded
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    dilate: (a boolean)
            Perform dilation rather than erosion
            flag: -dilate, position: 1
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    number_of_passes: (an integer)
            the number of passes (default: 1)
            flag: -npass %s
    out_filename: (a file name)
            Output image filename
            flag: %s, position: -1
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1

Outputs:

    out_file: (an existing file name)
            the output image

## GenerateWhiteMatterMask

Link to code

Wraps command gen_WM_mask

Generates a white matter probability mask from the DW images.

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> genWM = mrt.GenerateWhiteMatterMask()
    >>> genWM.inputs.in_file = 'dwi.mif'
    >>> genWM.inputs.encoding_file = 'encoding.txt'
    >>> genWM.run()

Inputs:

    [Mandatory]
    binary_mask: (an existing file name)
            Binary brain mask
            flag: %s, position: -2
    encoding_file: (an existing file name)
            Gradient encoding, supplied as a 4xN text file with each line is in
            the format [ X Y Z b ], where [ X Y Z ] describe the direction of
            the applied gradient, and b gives the b-value in units (1000
            s/mm^2). See FSL2MRTrix
            flag: -grad %s, position: 1
    in_file: (an existing file name)
            Diffusion-weighted images
            flag: %s, position: -3
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    noise_level_margin: (a float)
            Specify the width of the margin on either side of the image to be
            used to estimate the noise level (default = 10)
            flag: -margin %s
    out_WMProb_filename: (a file name)
            Output WM probability image filename
            flag: %s, position: -1

Outputs:

    WMprobabilitymap: (an existing file name)
            WMprobabilitymap

## MRConvert

Link to code

Wraps command mrconvert

Perform conversion between different file types and optionally extract a subset of the input image.

If used correctly, this program can be a very useful workhorse. In addition to converting images between different formats, it can be used to extract specific studies from a data set, extract a specific region of interest, flip the images, or to scale the intensity of the images.

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> mrconvert = mrt.MRConvert()
    >>> mrconvert.inputs.in_file = 'dwi_FA.mif'
    >>> mrconvert.inputs.out_filename = 'dwi_FA.nii'
    >>> mrconvert.run()

Inputs:

    [Mandatory]
    in_file: (an existing file name)
            voxel-order data filename
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    extension: ('mif' or 'nii' or 'float' or 'char' or 'short' or 'int'
             or 'long' or 'double', nipype default value: mif)
            "i.e. Bfloat". Can be "char", "short", "int", "long", "float" or
            "double"
    extract_at_axis: (1 or 2 or 3)
            "Extract data only at the coordinates specified. This option
            specifies the Axis. Must be used in conjunction with
            extract_at_coordinate.
            flag: -coord %s, position: 1
    extract_at_coordinate: (a list of from 1 to 3 items which are a
             float)
            "Extract data only at the coordinates specified. This option
            specifies the coordinates. Must be used in conjunction with
            extract_at_axis. Three comma-separated numbers giving the size of
            each voxel in mm.
            flag: %s, position: 2
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    layout: ('nii' or 'float' or 'char' or 'short' or 'int' or 'long' or
             'double')
            specify the layout of the data in memory. The actual layout produced
            will depend on whether the output image format can support it.
            flag: -output %s, position: 2
    offset_bias: (a float)
            Apply offset to the intensity values.
            flag: -scale %d, position: 3
    out_filename: (a file name)
            Output filename
            flag: %s, position: -1
    output_datatype: ('nii' or 'float' or 'char' or 'short' or 'int' or
             'long' or 'double')
            "i.e. Bfloat". Can be "char", "short", "int", "long", "float" or
            "double"
            flag: -output %s, position: 2
    prs: (a boolean)
            Assume that the DW gradients are specified in the PRS frame (Siemens
            DICOM only).
            flag: -prs, position: 3
    replace_NaN_with_zero: (a boolean)
            Replace all NaN values with zero.
            flag: -zero, position: 3
    resample: (a float)
            Apply scaling to the intensity values.
            flag: -scale %d, position: 3
    voxel_dims: (a list of from 3 to 3 items which are a float)
            Three comma-separated numbers giving the size of each voxel in mm.
            flag: -vox %s, position: 3

Outputs:

    converted: (an existing file name)
            path/name of 4D volume in voxel order

## MRMultiply

Link to code

Wraps command mrmult

Multiplies two images.

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> MRmult = mrt.MRMultiply()
    >>> MRmult.inputs.in_files = ['dwi.mif', 'dwi_WMProb.mif']
    >>> MRmult.run()

Inputs:

    [Mandatory]
    in_files: (an existing file name)
            Input images to be multiplied
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    out_filename: (a file name)
            Output image filename
            flag: %s, position: -1
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1

Outputs:

    out_file: (an existing file name)
            the output image of the multiplication

## MRTransform

Link to code

Wraps command mrtransform

Apply spatial transformations or reslice images

### Example

    >>> MRxform = MRTransform()
    >>> MRxform.inputs.in_files = 'anat_coreg.mif'
    >>> MRxform.run()

Inputs:

    [Mandatory]
    in_files: (an existing file name)
            Input images to be transformed
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    flip_x: (a boolean)
            assume the transform is supplied assuming a coordinate system with
            the x-axis reversed relative to the MRtrix convention (i.e. x
            increases from right to left). This is required to handle transform
            matrices produced by FSL's FLIRT command. This is only used in
            conjunction with the -reference option.
            flag: -flipx, position: 1
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    invert: (a boolean)
            Invert the specified transform before using it
            flag: -inverse, position: 1
    out_filename: (a file name)
            Output image
            flag: %s, position: -1
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1
    reference_image: (an existing file name)
            in case the transform supplied maps from the input image onto a
            reference image, use this option to specify the reference. Note that
            this implicitly sets the -replace option.
            flag: -reference %s, position: 1
    replace_transform: (a boolean)
            replace the current transform by that specified, rather than
            applying it to the current transform
            flag: -replace, position: 1
    template_image: (an existing file name)
            Reslice the input image to match the specified template image.
            flag: -template %s, position: 1
    transformation_file: (an existing file name)
            The transform to apply, in the form of a 4x4 ascii file.
            flag: -transform %s, position: 1

Outputs:

    out_file: (an existing file name)
            the output image of the transformation

## MRTrixViewer

Link to code

Wraps command mrview

Loads the input images in the MRTrix Viewer.

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> MRview = mrt.MRTrixViewer()
    >>> MRview.inputs.in_files = 'dwi.mif'
    >>> MRview.run()

Inputs:

    [Mandatory]
    in_files: (an existing file name)
            Input images to be viewed
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1

Outputs:

    None

## MedianFilter3D

Link to code

Wraps command median3D

Smooth images using a 3x3x3 median filter.

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> median3d = mrt.MedianFilter3D()
    >>> median3d.inputs.in_file = 'mask.mif'
    >>> median3d.run()

Inputs:

    [Mandatory]
    in_file: (an existing file name)
            Input images to be smoothed
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    out_filename: (a file name)
            Output image filename
            flag: %s, position: -1
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1

Outputs:

    out_file: (an existing file name)
            the output image

## Tensor2ApparentDiffusion

Link to code

Wraps command tensor2ADC

Generates a map of the apparent diffusion coefficient (ADC) in each voxel

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> tensor2ADC = mrt.Tensor2ApparentDiffusion()
    >>> tensor2ADC.inputs.in_file = 'dwi_tensor.mif'
    >>> tensor2ADC.run()

Inputs:

    [Mandatory]
    in_file: (an existing file name)
            Diffusion tensor image
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    out_filename: (a file name)
            Output Fractional Anisotropy filename
            flag: %s, position: -1
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1

Outputs:

    ADC: (an existing file name)
            the output image of the major eigenvectors of the diffusion tensor
            image.

## Tensor2FractionalAnisotropy

Link to code

Wraps command tensor2FA

Generates a map of the fractional anisotropy in each voxel.

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> tensor2FA = mrt.Tensor2FractionalAnisotropy()
    >>> tensor2FA.inputs.in_file = 'dwi_tensor.mif'
    >>> tensor2FA.run()

Inputs:

    [Mandatory]
    in_file: (an existing file name)
            Diffusion tensor image
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    out_filename: (a file name)
            Output Fractional Anisotropy filename
            flag: %s, position: -1
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1

Outputs:

    FA: (an existing file name)
            the output image of the major eigenvectors of the diffusion tensor
            image.

## Tensor2Vector

Link to code

Wraps command tensor2vector

Generates a map of the major eigenvectors of the tensors in each voxel.

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> tensor2vector = mrt.Tensor2Vector()
    >>> tensor2vector.inputs.in_file = 'dwi_tensor.mif'
    >>> tensor2vector.run()

Inputs:

    [Mandatory]
    in_file: (an existing file name)
            Diffusion tensor image
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    out_filename: (a file name)
            Output vector filename
            flag: %s, position: -1
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1

Outputs:

    vector: (an existing file name)
            the output image of the major eigenvectors of the diffusion tensor
            image.

## Threshold

Link to code

Wraps command threshold

Create bitwise image by thresholding image intensity.

By default, the threshold level is determined using a histogram analysis to cut out the background. Otherwise, the threshold intensity can be specified using command line options. Note that only the first study is used for thresholding.

### Example

    >>> import nipype.interfaces.mrtrix as mrt
    >>> thresh = mrt.Threshold()
    >>> thresh.inputs.in_file = 'wm_mask.mif'
    >>> thresh.run()

Inputs:

    [Mandatory]
    in_file: (an existing file name)
            The input image to be thresholded
            flag: %s, position: -2
    terminal_output: ('stream' or 'allatonce' or 'file' or 'none')
            Control terminal output: `stream` - displays to terminal
            immediately, `allatonce` - waits till command is finished to display
            output, `file` - writes output to file, `none` - output is ignored

    [Optional]
    absolute_threshold_value: (a float)
            Specify threshold value as absolute intensity.
            flag: -abs %s
    args: (a string)
            Additional parameters to the command
            flag: %s
    debug: (a boolean)
            Display debugging messages.
            flag: -debug, position: 1
    environ: (a dictionary with keys which are a value of type 'str' and
             with values which are a value of type 'str', nipype default value:
             {})
            Environment variables
    ignore_exception: (a boolean, nipype default value: False)
            Print an error message instead of throwing an exception in case the
            interface fails to run
    invert: (a boolean)
            Invert output binary mask
            flag: -invert, position: 1
    out_filename: (a file name)
            The output binary image mask.
            flag: %s, position: -1
    percentage_threshold_value: (a float)
            Specify threshold value as a percentage of the peak intensity in the
            input image.
            flag: -percent %s
    quiet: (a boolean)
            Do not display information messages or progress status.
            flag: -quiet, position: 1
    replace_zeros_with_NaN: (a boolean)
            Replace all zero values with NaN
            flag: -nan, position: 1

Outputs:

    out_file: (an existing file name)
            The output binary image mask.